Ironwood  Spec List 

Stage size  16'x20' with 8'x8'x1' drm. riser, plus 2 side riser's

Main Mix Console  - Midas M- 32 
Main speaker's 4 EV -  15"x1"    1 EV - Dbl. 18
Stage Monitors 4 EV - 12"x1"     1 JBL - 15"x2" drm fill. 

Microphones - 4 Sennheiser  835 vocal mic  -  8 Sure 58  -  3 Sure 57   - 3 Sure 57A   - 2 Sennheiser 609   - 5 Sennheiser 604   - 2 JM27 condenser   -  2 Sure sm81  -  3 AudioTechnica 350s   - 1 Beta 52  -  1 PG 52 - 1 Sennheiser 421 - 1 AKG C 1000 
 
Direct Boxes -1 Radial JDI 2ch -   1 Radial JDI   - 2 Radial J48  -  1 Radial Pro 48   - 2 Klark D100
 
All cables and stands  to suport above  Plus 6 guitar stands 1 Keyboard stand We supply 5 wedge monitor mix's   We do not supply any back line 
 
System can produce 115db of clean power, more than the size of the venue needs More monitors or back line can be rented at  Performer's Cost 
 
any more tech info please text or call   JT@403-554-6037          jtsndeng@gmail.com